Act, Sec. 67 **PAPUA NEW GUINEA** Form 10

Reg., Sec.19 ***(TRADE MARKS ACT (CHAPTER 385)***

# APPLICATION FOR CANCELLATION OF REGISTRATION OF REGISTERED USER

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | |  | FOR OFFICIAL USE | | |
| PAYMENT BY BANK DRAFT  OR CHEQUE ACCEPTED  FEE:  ITEM 19 | |  |  | | |
| 1. Insert the full name   name of the individual,  firm or body corporate  making application. If | | Application  is hereby  made by (a) | |  | | |
| a boby corporate, firm or  analogous body is making  application, indicate the  State or country of  incorporation or registra-  tion. The names of all  parties in a firm must be  given in full | | |  |  | | |
| 1. Here insert the   full trade or business  of the applicant. | | | whose trade  or business  address is  (b) |  | | |
|  | | |  |  | |
| 1. Here insert full for cancellation of the following   name and other details Registered User  sufficient to identify  the Registered User | | | | | |
|  | | | |
| (d) Here insert the in respect of  number of the Registered Registered  Trade Mark. Trade Mark No.  (d) | | | | |  |

|  |  |  |
| --- | --- | --- |
|  | My/Our address  for service in  Papua New Guinea  is |  |
|  |  | |

(e) Insert date.

A copy of this notice was served on ……………………………………………… (e)

On the proprietor/applicant in accordance with Regulation Section 45.

……………………… ……………………………..

Signature Date

**NOTE:**

1. Any document submitted to the Registrar (other than a prescribed form) shall be written on one side only.
2. Any other document submitted to the Registrar shall :
3. be written in a permanent ink on which bleaching agents do not have any effect;
4. have margins of not less than 25mm on the left-hand side and 12mm on right-hand side;
5. be of international A4 size;
6. be handwritten or printed in type of not less than 12 point;
7. be on durable white paper, the thickness of 300 sheets of not less than 25mm; and
8. be securely bound together where a document comprises of more than 2 sheets and shall have a margin of not less than 25mm on the sideon which it is bound.